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Removal of bacteriophages MS2 and ΦX174 in biotic iron and manganese filters and in ultrafiltration of iron and manganese containing backwash water
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Figure SI1: Concentration of MS2 phage in feed and permeate samples of Fe-FSW during UF at different membrane fluxes. Dashed grey line indicates the LOQ (2 PFU/100 mL) and an asterisk indicates samples were below LOQ and set to LOQ for calculations and display.
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